Technical data

| Operating voltage | 8 – 30 V |
| --- | --- |
| Current consumption | < 3 mA |
| Switching current | 16 A (at 24 V) |
| Ambient temperature | -20 °C – +50 °C |
| Dimensions (W × H × D) | 150 × 40 × 50 mm |
| Weight | 0.153 g approx. |
| Item numbers | AkkuGuard – A: 30015 AkkuGuard – U: 30017 |

This technical data sheet has been created to the best of the author’s knowledge. Duplication of these instructions or parts thereof by any reproduction method whatsoever is prohibited without the prior permission of Industrieelektronik Pölz GmbH. This technical data sheet does not represent a contractual relationship. We reserve the right to make changes errors and omissions excepted. © Copyright 2017 Industrieelektronik Pölz GmbH