Technical data

| Mains voltage(s)/type of current | 2 × 12 V DC in-series (24 V) |
| --- | --- |
| Current consumption | 3 A max. |
| Degree of protection | IP56 |
| Ambient temperature | -40 °C / +85 °C |
| Degree of effectiveness | ~85 % |
| No-load current | 0.9 mA |
| Operating current | 0 – 3 A |
| Protection against polarity reversal | Yes |
| Short circuit-protection | Yes |
| Load disconnection | via relay |
| Dimensions (L x W x H) | 115 × 60 × 35 mm |
| Weight | 0.247 kg approx. |
| Item number | 30058 |

This technical data sheet has been created to the best of the author’s knowledge. Duplication of these instructions or parts thereof by any reproduction method whatsoever is prohibited without the prior permission of Industrieelektronik Pölz GmbH. This technical data sheet does not represent a contractual relationship. We reserve the right to make changes errors and omissions excepted. © Copyright 2017 Industrieelektronik Pölz GmbH