Technical data

| Dimensions (W × H × D) | 220 × 160 × 55 mm |
| --- | --- |
| Weight | 1 kg approx. |
| Power supply | 6 V / DC  |
| Battery type | AA/LR6, 1.5 V, 1500 mAh |
| Current consumption | 170 mA |
| Current consumption with display lighting switched off | 50 mA |
| Maximum operating time | 16 hrs. |
| Average operating time | 8 hrs. |
| Time for changing batteries (without losing data) | 15 min. |
| Alarm | 90 dB max. at 1 m |
| Ambient temperature | -20 °C / +70 °C |
| Item numbers | Checkbox 5+1 SERIAL: 30158Checkbox 5+1 USB V04: 30936Checkbox 5+1 USB: 30160 |

This technical data sheet has been compiled to the best of our knowledge and belief. Duplication of these instructions or parts thereof by any reproduction method whatsoever is prohibited without the prior permission of Industrieelektronik Pölz GmbH. This technical data sheet does not constitute a document with contractual character. We reserve the right to make changes errors and omissions excepted. © Copyright 2017 Industrieelektronik Pölz GmbHw